{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["691 B Belts cross","691 sources","description","Sheet5"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"691 B Belts cross","index":0,"n_rows":79,"n_cols":12,"rows_kept":79,"cut":false,"hidden":false,"merged":[]}
["No.","Category number","Category name","NSC SKU","NSC Description","Long description","Gates\nSKU","Jason\nSKU","Dayco\nSKU","Mars\nSKU ","5L belts number \n(B belts are similar to 5L)","Notes"]
[1,691,"B-BELTS",90032023,"691 - B-23,GATES(HI-POWER)BELT","B23 V-Belt, B/5L Section \nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 26.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B23","B23 (5L260)","BP23",94419,"5L260","1. Dayco SKU is assumed\n2. we have this belt on hand from Mars "]
[2,691,"B-BELTS","90032028","691 - B-28,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B28 Hi-Power II V-Belt - 9003-2028. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):31.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B28","B28 (5L310)","BP28",null,"5L310"]
[3,691,"B-BELTS","90032030","691 - B-30,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B30 Hi-Power II V-Belt - 9003-2030.  Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):33. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B30","B30 (5L330)","BP30",94422,"5L330"]
[4,691,"B-BELTS","90032031","691 - B-31,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B31 Hi-Power II V-Belt - 9003-2031. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 34. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B31","B31 (5L340)","BP31",94423,"5L340"]
[5,691,"B-BELTS","90032032","691 - B-32,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B32 Hi-Power II V-Belt - 9003-2032. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 35 \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B32","B32 (5L350)","BP32",94424,"5L350"]
[6,691,"B-BELTS","90032033","691 - B-33,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B33 Hi-Power II V-Belt - 9003-2033. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):36.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B33","B33 (5L360)","BP33",94425,"5L360"]
[8,691,"B-BELTS","90032035","691 - B-35,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II \nGates B35 Hi-Power II V-Belt - 9003-2035 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  38. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B35","B35 (5L380)","BP35",94427,"5L380"]
[9,691,"B-BELTS","90032036","691 - B-36,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B36 Hi-Power II V-Belt - 9003-2036. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):39. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B36","B36 (5L390)","BP36",94428,"5L390"]
[10,691,"B-BELTS","90032037","691 - B-37,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B37 Hi-Power II V-Belt - 9003-2037. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):40. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B37","B37 (5L400)","BP37",94429,"5L400"]
[11,691,"B-BELTS","90032038","691 - B-38,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B38 Hi-Power II V-Belt - 9003-2038 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  41. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B38","B38 (5L410)","BP38",94430,"5L410"]
[12,691,"B-BELTS","90032039","691 - B-39,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B39 Hi-Power II V-Belt - 9003-2039. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):42.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B39","B39 (5L420)","BP39",94431,"5L420"]
[13,691,"B-BELTS","90032040","691 - B-40,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B40 Hi-Power II V-Belt - 9003-2040 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  43. \nThese belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B40","B40 (5L430)","BP40",94432,"5L430"]
[14,691,"B-BELTS","90032041","691 - B-41,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B41 V-belt Hi-Power II V-Belt - 9003-2041. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 44.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B41","B41 (5L440)","BP41",94433,"5L440"]
[15,691,"B-BELTS","90032042","691 - B-42,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates\nB42 Hi-Power II V-Belt - 9003-2042 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  45.\nThese belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B42","B42 (5L450)","BP42",94434,"5L450"]
[16,691,"B-BELTS","90032043","691 - B-43,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates\nB43 Hi-Power II V-Belt - 9003-2043 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  46. \nThese belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B43","B43 (5L460)","BP43",94435,"5L460"]
[17,691,"B-BELTS","90032044","691 - B-44,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II \nGates B44 Hi-Power II V-Belt - 9003-2044 Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  47.\nThese belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B44","B44 (5L470)","BP44",94436,"5L470"]
[18,691,"B-BELTS","90032045","691 - B-45,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B45 Hi-Power II V-Belt - 9003-2045. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):48. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B45","B45 (5L480)","BP45",94437,"5L480"]
[19,691,"B-BELTS","90032046","691 - B-46,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B46 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 49 \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B46","B46 (5L490)","BP46",94438,"5L490"]
[20,691,"B-BELTS","90032047","691 - B-47,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B47 V-belt Hi-Power II V-Belt - 9003-2047. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 50. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B47","B47 (5L500)","BP47",94439,"5L500"]
[21,691,"B-BELTS","90032048","691 - B-48,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B48 Hi-Power II V-Belt Belt - 9003-2048. Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 51 \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B48","B48 (5L510)","BP48",94440,"5L510"]
[22,691,"B-BELTS","90032049","691 - B-49,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B49 Hi-Power II V-Belt - 9003-2049. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):52. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B49","B49 (5L520)","BP49",94441,"5L520"]
[23,691,"B-BELTS","90032050","691 - B-50,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B50 Hi-Power II V-Belt Belt - 9003-2050. Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 53.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B50","B50 (5L530)","BP50",94442,"5L530"]
[24,691,"B-BELTS","90032051","691 - B-51,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B51 Hi-Power II V-Belt - 9003-2051. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):54. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B51","B51 (5L540)","BP51",94443,"5L540"]
[25,691,"B-BELTS","90032052","691 - B-52,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B52 Hi-Power II V-Belt - 9003-2052. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):55. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B52","B52 (5L550)","BP52",94444,"5L550"]
[26,691,"B-BELTS","90032053","691 - B-53,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B53 Hi-Power II V-Belt - 9003-2053. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):56. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B53","B53 (5L560)","BP53",94445,"5L560"]
[27,691,"B-BELTS","90032054","691 - B-54,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B54 Hi-Power II V-Belt - 9003-2054. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):57. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B54","B54 (5L570)","BP54",94446,"5L570"]
[28,691,"B-BELTS","90032055","691 - B-55,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B55 Hi-Power II V-Belt - 9003-2055. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):58. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B55","B55 (5L580)","BP55",94447,"5L580"]
[29,691,"B-BELTS","90032056","691 - B-56,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B56 Hi-Power II V-Belt - 9003-2056. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):59. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B56","B56 (5L590)","BP56",94448,"5L590"]
[30,691,"B-BELTS","90032057","691 - B-57,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B57 Hi-Power II V-Belt - 9003-2057. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 60.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B57","B57 (5L600)","BP57",94449,"5L600"]
[31,691,"B-BELTS","90032058","691 - B-58,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B58 V-belt Hi-Power II V-Belt - 9003-2058. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 61. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B58","B58 (5L610)","BP58",94450,"5L610"]
[32,691,"B-BELTS","90032059","691 - B-59,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B59 Hi-Power II V-Belt - 9003-2059. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):62. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B59","B59 (5L620)","BP59",94451,"5L620"]
[33,691,"B-BELTS","90032060","691 - B-60,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B60 Hi-Power II V-Belt - 9003-2060. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 63. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B60","B60 (5L630)","BP60",94452,"5L630"]
[34,691,"B-BELTS","90032061","691 - B-61,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B61 V-belt Hi-Power II V-Belt - 9003-2061. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 64. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B61","B61 (5L640)","BP61",94453,"5L640"]
[35,691,"B-BELTS","90032062","691 - B-62,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B62 V-belt Hi-Power II V-Belt - 9003-2062. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 65. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B62","B62 (5L650)","BP62",94454,"5L650"]
[36,691,"B-BELTS","90032063","691 - B-63,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B63 V-belt Hi-Power II V-Belt - 9003-2063. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 66. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B63","B63 (5L660)","BP63",94455,"5L660"]
[37,691,"B-BELTS","90032064","691 - B-64,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B64 V-belt Hi-Power II V-Belt - 9003-2064. Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  67.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B64","B64 (5L670)","BP64",94456,"5L670"]
[38,691,"B-BELTS","90032065","691 - B-65,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B65 Hi-Power II V-Belt - 9003-2065. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):68. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B65","B65 (5L680)","BP65",94457,"5L680"]
[39,691,"B-BELTS","90032066","691 - B-66,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B66 Hi-Power II V-Belt - 9003-2066. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):69. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B66","B66 (5L690)","BP66",94458,"5L690"]
[40,691,"B-BELTS","90032067","691 - B-67,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B67 Hi-Power II V-Belt - 9003-2067. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):70. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B67","B67 (5L700)","BP67",94459,"5L700"]
[41,691,"B-BELTS","90032068","691 - B-68,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B68 Hi-Power II V-Belt - 9003-2068. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):71. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B68","B68 (5L710)","BP68",94460,"5L710"]
[42,691,"B-BELTS","90032069","691 - B-69,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B69 Hi-Power II V-Belt - 9003-2069. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):72. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B69","B69 (5L720)","BP69",94461,"5L720"]
[43,691,"B-BELTS","90032070","691 - B-70,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B70 V-belt Hi-Power II V-Belt - 9003-2070. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 73. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B70","B70 (5L730)","BP70",94462,"5L730"]
[44,691,"B-BELTS","90032071","691 - B-71,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B71 Hi-Power II V-Belt - 9003-2071. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):74. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B71","B71 (5L740)","BP71",94463,"5L740"]
[45,691,"B-BELTS","90032072","691 - B-72,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B72 Hi-Power II V-Belt - 9003-2072. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):75. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B72","B72 (5L750)","BP72",94464,"5L750"]
[46,691,"B-BELTS","90032073","691 - B-73,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B73 V-belt Hi-Power II V-Belt - 9003-2073. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 76. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B73","B73 (5L760)","BP73",94465,"5L760"]
[47,691,"B-BELTS","90032074","691 - B-74,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B74 Hi-Power II V-Belt - 9003-2074. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):77. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B74","B74 (5L770)","BP74",94466,"5L770"]
[48,691,"B-BELTS","90032075","691 - B-75,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B75 Hi-Power II V-Belt - 9003-2075. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):78. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B75","B75 (5L780)","BP75",94467,"5L780"]
[49,691,"B-BELTS","90032076","691 - B-76,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B76 Hi-Power II V-Belt - 9003-2076. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):79. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B76","B76 (5L790)","BP76",94468,"5L790"]
[50,691,"B-BELTS","90032077","691 - B-77,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B77 Hi-Power II V-Belt - 9003-2077. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):80. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B77","B77 (5L800)","BP77",94469,"5L800"]
[51,691,"B-BELTS","90032078","691 - B-78,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B78 Hi-Power II V-Belt - 9003-2078. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):81. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B78","B78 (5L810)","BP78",94470,"5L810"]
[52,691,"B-BELTS","90032079","691 - B-79,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B79 Hi-Power II V-Belt - 9003-2079. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):82. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B79","B79 (5L820)","BP79",94471,"5L820"]
[53,691,"B-BELTS","90032080","691 - B-80,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B80 Hi-Power II V-Belt - 9003-2080. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):83. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B80","B80 (5L830)","BP80",94472,"5L830"]
[54,691,"B-BELTS","90032081","691 - B-81,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B81 Hi-Power II V-Belt - 9003-2081. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):84. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B81","B81 (5L840)","BP81",94473,"5L840"]
[55,691,"B-BELTS","90032082","691 - B-82,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B82 Hi-Power II V-Belt - 9003-2082. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):85. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B82","B82 (5L850)","BP82",94474,"5L850"]
[58,691,"B-BELTS","90032083","691 - B-83,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B83 Hi-Power II V-Belt - 9003-2083. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 86. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B83","B83 (5L860)","BP83",94475,"5L860"]
[59,691,"B-BELTS","90032084","691 - B-84,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B84 Hi-Power II V-Belt - 9003-2084. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 87. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B84","B84 (5L870)","BP84",94476,"5L870"]
[60,691,"B-BELTS","90032085","691 - B-85,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B85 Hi-Power II V-Belt - 9003-2085. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 88. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B85","B85 (5L880)","BP85",94477,"5L880"]
[61,691,"B-BELTS","90032086","691 - B-86,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B86 Hi-Power II V-Belt - 9003-2086. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 89. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B86","B86 (5L890)","BP86",94478,"5L890"]
[62,691,"B-BELTS",90032087,"691 - B-87,GATES(HI-POWER)BELT","B87 V-Belt, B/5L Section \nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 90.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B87","B87 (5L900)","BP87",94479,"5L900","\nwe have this belt on hand from Mars "]
[63,691,"B-BELTS","90032088","691 - B-88,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B88 Hi-Power II V-Belt - 9003-2088. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 91. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B88","B88 (5L910)","BP88",94480,"5L910"]
[64,691,"B-BELTS",90032089,"691 - B-89,GATES(HI-POWER)BELT","B89 V-Belt\nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 92.\nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B89","B89 (5L920)","BP89",94481,"5L920","\nwe have this belt on hand from Dayco "]
[65,691,"B-BELTS","90032090","691 - B-90,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B90 Hi-Power II V-Belt - 9003-2090. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 93. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B90","B90 (5L930)","BP90",94482,"5L930"]
[66,691,"B-BELTS","90032093","691 - B-93 GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B93 Hi-Power II V-Belt - 9003-2093. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 96. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B93","B93 (5L960)","BP93",94484,"5L960"]
[67,691,"B-BELTS","90032094","691 - B-94,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B94 Hi-Power II V-Belt - 9003-2094. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 97. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B94","B94 (5L970)","BP94",94485,"5L970"]
[68,691,"B-BELTS","90032097","691 - B-97,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B97 Hi-Power II V-Belt - 9003-2097. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 100. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B97","B97 (5L1000)","BP97",94488,"5L1000"]
[69,691,"B-BELTS","90032105","691 - B-105,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B105 Hi-Power II V-Belt - 9003-2105. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 108. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B105","B105","BP105",94493,""]
[70,691,"B-BELTS","90032106","691 - B-106,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B106 Hi-Power II V-Belt - 9003-2106. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 109. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B106","B106 ","BP106",94494,""]
[71,691,"B-BELTS","90032108","691 - B-108,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B108 Hi-Power II V-Belt - 9003-2108. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):111. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B108","B108","BP108",94495,""]
[72,691,"B-BELTS","90032118","691 - B-118,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B118 V-belt Hi-Power II V-Belt - 9003-2118. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 121. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B118","B118","BP118",94500,""]
[73,691,"B-BELTS","90032120","691 - B-120,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B120 V-belt Hi-Power II V-Belt - 9003-2120. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 123. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B120","B120","BP120",94501,""]
[74,691,"B-BELTS","90032124","691 - B-124,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B124 V-belt Hi-Power II V-Belt - 9003-2124. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 127. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B124","B124","BP124",94502,""]
[75,691,"B-BELTS","90032128","691 - B-128 GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B128 V-belt Hi-Power II V-Belt - 9003-2128. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 131. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B128","B128","BP128",94504,""]
[76,691,"B-BELTS","90032131","691 - B-131,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B131 V-belt Hi-Power II V-Belt - 9003-2131. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 133. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B131","B131","BP131",null,""]
[77,691,"B-BELTS","90032136","691 - B-136,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B136 V-belt Hi-Power II V-Belt - 9003-2136. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 139. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B136","B136","BP136",94506,""]
[78,691,"B-BELTS","90032158","691 - B-158,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B158 V-belt Hi-Power II V-Belt - 9003-2158. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 161. \nThese belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.","B158","B158","BP158",94512,""]
[79,691,"B-BELTS",90032025,"695 - B-25 JASON HI-POWER BELT","B25 / B Section Classical V-Belts \nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 28.","B25","B25 (5L280)","BP25",94421,"5L280","on hand only in Timmins"]
[80,691,"B-BELTS",90032029,"696 - B-29 JASON HI-POWER BELT","B29 / B Section Classical V-Belts \nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 32.","B29","B29 (5L320)","BP29",null,"5L320","on hand only in Timmins"]
[81,691,"B-BELTS",90032034,"697 - B-34 JASON HI-POWER BELT","B34 / B Section Classical V-Belts \nBelt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 37.","B34","B34 (5L370)","BP34",94426,"5L370","on hand only in Timmins"]

{"sheet":"691 sources","index":1,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Manufacturer","Source 1 of SKU search","Source 2 of SKU search"]
["Gates","https://www.vbelts4less.com/standard-a-series-v-belt ","https://www.gates.com/us/en/search.html?searchType=product&text=hi+power "]
["Jason","https://www.jasonindustrial.com/wp-content/uploads/HVAC-R-Product-Guide.pdf "]
["Dayco","https://www.vbelts4less.com/standard-a-series-v-belt "]
["Mars","https://fergusonprod.a.bigcontent.io/v1/static/3927249_3919284_specification","https://www.marsdelivers.com/wps/wcm/connect/5e2e8bf2-2fb9-495b-8151-a47c1ec04914/V-Belts.pdf?MOD=AJPERES&CONVERT_TO=url&CACHEID=5e2e8bf2-2fb9-495b-8151-a47c1ec04914 "]

{"sheet":"description","index":2,"n_rows":185,"n_cols":7,"rows_kept":185,"cut":false,"hidden":false,"merged":[]}
["SKU (50 max) *","Short Description (255 max) *","Long Description (255 max)"]
["941+A15:A18600","MARS BELT SIZER","Measure FHP Belts upto 107\" to determine equivalent Truflex belts numbers",null,"MARS"]
[94419,"B-23,MARS V-BELT","B23 V-Belt, Consumer Brand. 21/32” (5/8”) Wide \nx 26” Length OC (Metric 16mm W x 660mm La). \nStatic, Heat, and Oil resistant. High quality for low cost!",null,"B-23",{"$f":"SUBSTITUTE(E3,\"-\",\"\")","v":"B23"}]
[408603,"V-BELT DRESSING 11oz. AEROSOL(6/BX)","Eliminates squeaks and prolongs belt life. For\n use on all types of belts, such as serpentine,\n flat and v-type belts. Prevents slippage and \nglazing. Removes oil, grease and glaze",null,"V-BELT",{"$f":"SUBSTITUTE(E4,\"-\",\"\")","v":"VBELT"}]
[74217,"4L-780,GATES(TRUFLEX)BELT","4L780 Gates Truflex light duty v-belt 78 inches long x 1/2 top width.",null,"4L-780","4L780"]
["BX42","BX42 BELT 42\" COGGED","For industrial drives. Rubber Impregnated Fabric.\n Datum Length:43.8\". Outer Length:45\". Section: BX.\n Series: BX42. Thickness:13/32\". Type: Cogged V-Belt.\n Width: 21/32\", Product Weight:0.43",null,"BX42","BX42"]
["BX47","BX47 BELT 47\" COGGED","21/32\" Top Width X 50\" Outside Measurement.\n Manufacturer Part#: BX47. TECHNICAL \nSPECIFICATIONS: Series: BX47 Cogged V-Belt.\n Widths: 21/32 Inch, (17mm). Outside Length:\n 50 Inch, Inside Length: 47 Inch, Material: Neoprene",null,"BX47","BX47"]
["BX48","BX48 BELT 48\" COGGED","Item Cogged V-Belt. V-Belt Type Cogged V-Belt.\n V-Belt Section BX . Industry Number: BX48. \nNumber of Ribs 1. Outside Length 51\" .Top Width 21/32\" Thickness 3/32\" Material Fabric Cover, Rubber Body, Polyester Cords Construction Raw Edge, Cogged Temp. Range -22 Degrees to 194 Degrees F Resists Heat, Oil",null,"BX48","BX48"]
["ALINK5","A LINK BELT 5FT LENGTH","",null,"A","A"]
[84001190,"3L-190,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 3L190 8400-1190. Truflex® belts feature superior length stability for minimal take-up. 3L190 Gates Truflex light duty v-belt 19 inches long x 3/8 top width. Gates product ID 84001190 Belt Height:  7/32 Belt Top Width:  3/8 Outside Circumference (in): 19",null,"3L-190","3L190"]
[84001210,"3L-210,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 3L210 8400-1210 3L210 Gates Truflex light duty v-belt 21 inches long x 3/8 top width.  Belt Height:  7/32Belt Top Width:  3/8 Outside Circumference (in): 21",null,"3L-210","3L210"]
[84002200,"4L-200,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light\n duty v-belt 4L200 8400-2200. 4L200 Gates Truflex light duty v-belt 20 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2Outside Circumference (in):  20",null,"4L-200","4L200"]
[84002210,"4L-210,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L210 8400-2210 4L210 Gates Truflex light duty v-belt 21 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 21",null,"4L-210","4L210"]
[84002220,"4L-220,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L220 8400-2220. \n4L220 Gates Truflex light duty v-belt 22 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 22\nMPN: 4L220",null,"4L-220","4L220"]
[84002240,"4L-240,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L240 8400-2240\n4L240 Gates Truflex light duty v-belt 24 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 24 MPN:  4L240",null,"4L-240","4L240"]
[84002250,"4L-250,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L250 8400-2250. 4L250 Gates Truflex light duty v-belt 25 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 25 MPN:  4L250\n",null,"4L-250","4L250"]
[84002280,"4L-280,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L280 8400-2280. 4L280 Gates Truflex light duty v-belt 28 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 28 MPN:  4L280",null,"4L-280","4L280"]
[84002290,"4L-290,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L290 8400-2290. \n4L290 Gates Truflex light duty v-belt 29 inches long x 1/2 top width.\nBelt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in):  29\nMPN:  4L290",null,"4L-290","4L290"]
[84002340,"4L-340,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD.Gates Truflex light duty v-belt 4L340 8400-2340.\n4L340 Gates Truflex light duty v-belt 34 inches long x 1/2 top width. \nBelt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in):  34\nMPN:  4L340",null,"4L-340","4L340"]
[90032064,"B-64,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B64 Hi-Power II V80 Series Vbelt. these belts resist oil and heat, ozone, sunlight, weather, and aging.Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  67\nMPN:  B64 .Meets ARPM / RMA IP-3-2 oil and heat-resistant standards.\nMeets ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-64","B64"]
[90032067,"B-67,GATES(HI-POWER)BELT","Gates B64 Hi-Power II V-Belt - 9003-2064.Belt Height:  13/32\nBelt Top Width:  21/32.Outside Circumference (in):  67\nMPN:  B64 these belts resist oil and heat, ozone, sunlight, weather, and aging.\nMeets ARPM / RMA IP-3-2 oil and heat-resistant standards.Meets ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-67","B67"]
[90032088,"B-88,GATES(HI-POWER)BELT","Gates B88 Hi-Power II V80 Series Vbelt Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  91 Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-88","B88"]
[90032034,"B-34,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B34 Hi-Power II V-Belt - 9003-2034\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  37\nMeets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements",null,"B-34","B34"]
[90032035,"B-35,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B35 Hi-Power II V-Belt - 9003-2035\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  38. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-35","B35"]
[90032038,"B-38,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B38 Hi-Power II V-Belt - 9003-2038\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  41. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-38","B38"]
[90032040,"B-40,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B40 Hi-Power II V-Belt - 9003-2040\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  43. These belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-40","B40"]
[90032042,"B-42,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B42 Hi-Power II V-Belt - 9003-2042\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  45. These belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-42","B42"]
[90032044,"B-44,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II Gates B44 Hi-Power II V-Belt - 9003-2044\nBelt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  47.These belts resist oil and heat, ozone, sunlight, weather, and aging. ",null,"B-44","B44"]
[90032046,"B-46,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B46 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 49 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-46","B46"]
[90032048,"B-48,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B48 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 51 These belts resist oil, heat, ozone,\n sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-48","B48"]
[90032050,"B-50,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B50 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 53 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-50","B50"]
[90032057,"B-57,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B57 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 57 These belts resist oil, heat, ozone,\nsunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-57","B57"]
[90022026,"A-26,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A26 Hi-Power II V80  Series. Belt outside circumference length of 28 inches.  Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 28 These belts resist oil, heat, ozone,\nsunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-26","A26","A26"]
[90022027,"A-27,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A27 Hi-Power II V80  Series. Belt outside circumference length of 29 inches.  Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 29 These belts resist oil, heat, ozone,\nsunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-27","A27","A27"]
[90022030,"A-30,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A30 V-belt Hi-Power II V80 Series. Belt outside circumference length of 32 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 32 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-30","A30","A30"]
[90022031,"A-31, GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A31 V-belt Hi-Power II V80 Series. Belt outside circumference length of 33 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 33 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-31","A31","A31"]
[90022032,"A-32,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A32 V-belt Hi-Power II V80 Series. Belt outside circumference length of 34 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 34. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-32","A32","A32"]
[90022033,"A-33,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A33 V-belt Hi-Power II V80 Series. Belt outside circumference length of 35 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 35. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-33","A33","A33"]
[90022034,"A-34,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A34 V-belt Hi-Power II V80 Series. Belt outside circumference length of 36 inches. Belt Height: 5/16 Belt Top Width: 1/2\nOutside Circumference (in): 36. These belts resist oil, heat, ozone,\nsunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-34","A34","A34"]
[90022035,"A-35,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A35 V-belt Hi-Power II V80 Series. Belt outside circumference length of 37 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 37. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-35","A35","A35"]
[90022036,"A-36,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A36 V-belt Hi-Power II V80 Series. Belt outside circumference length of 38 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 38. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-36","A36","A36"]
[90022037,"A-37,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A37 V-belt Hi-Power II V80 Series. Belt outside circumference length of 39 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 39. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-37","A37","A37"]
[90022038,"A-38,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A38 V-belt Hi-Power II V80 Series. Belt outside circumference length of 40 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 40. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and  heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-38","A38","A38"]
[90022039,"A-39,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A39 V-belt Hi-Power II V80 Series. Belt outside circumference length of 41 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 41. These belts resist oil, heat, ozone,sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-39","A39","A39"]
[90022040,"A-40,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A40 V-belt Hi-Power II V80 Series. Belt outside circumference length of 42 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 42. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-40","A40","A40"]
[90022042,"A-42,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A42 V-belt Hi-Power II V80 Series. Belt outside circumference length of 44 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 44. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-42","A42","A42"]
[90022043,"A-43,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A43 V-belt Hi-Power II V80 Series. Belt outside circumference length of 45 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 45. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-43","A43","A43"]
[90022044,"A-44,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A44 V-belt Hi-Power II V80 Series. Belt outside circumference length of 46 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 46. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-44","A44","A44"]
[90022045,"A-45,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A45 V-belt Hi-Power II V80 Series. Belt outside circumference length of 47 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 47. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and  heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-45","A45","A45"]
[90022046,"A-46,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A46 V-belt Hi-Power II V80 Series. Belt outside circumference length of 48 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 48. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-46","A46","A46"]
[90022047,"A-47,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A47 V-belt Hi-Power II V80 Series. Belt outside circumference length of 49 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 49. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-47","A47","A47"]
[90022048,"A-48,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD IIHi-Power® II Belts / Courroies Hi-PowerMD II\nGates A48 V-belt Hi-Power II V80 Series. Belt outside circumference length of 50 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 50. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-48","A48","A48"]
[90022049,"A-49 GATES(HI-POWER) BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A49 V-belt Hi-Power II V80 Series. Belt outside circumference length of 51 inches. Belt Height: 5/16 Belt Top Width: 1/2\nOutside Circumference (in): 51. These belts resist oil, heat, ozone,\nsunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-49","A49","A49"]
[90022050,"A-50,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A50 V-belt Hi-Power II V80 Series. Belt outside circumference length of 52 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 52. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-50","A50","A50"]
[90022051,"A-51,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A51 V-belt Hi-Power II V80 Series. Belt outside circumference length of 53 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 53. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-51","A51","A51"]
[90022052,"A-52,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A52 V-belt Hi-Power II V80 Series. Belt outside circumference length of 54 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 54. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-52","A52","A52"]
[90022053,"A-53,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A53 V-belt Hi-Power II V80 Series. Belt outside circumference length of 55 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 55. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-53","A53","A53"]
[90022054,"A54 GATES HI POWER BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A54 V-belt Hi-Power II V80 Series. Belt outside circumference length of 56 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 56. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A54","A54","A54"]
[90022055,"A-55,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A55 V-belt Hi-Power II V80 Series. Belt outside circumference length of 57 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 57. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-55","A55","A55"]
[90022056,"A-56,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A56 V-belt Hi-Power II V80 Series. Belt outside circumference length of 58 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 58. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-56","A56","A56"]
[90022062,"A-62,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A62 V-belt Hi-Power II V80 Series. Belt outside circumference length of 64 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 64. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-62","A62","A62"]
[84002190,"4L190 GATES (TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L190 8400-2190.  4L190 Gates Truflex light duty v-belt 19 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in):  19 MPN:  4L190",null,"4L190","4L190","A29"]
[84002360,"4L-360,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L360 8400-2360.  4L360 Gates Truflex light duty v-belt 36 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 36 MPN:  4L360",null,"4L-360","4L360","A41"]
[84002430,"4L-430,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L430 8400-2430. \n4L430 Gates Truflex light duty v-belt 43 inches long x 1/2 top width. Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 43\nMPN:  4L430",null,"4L-430","4L430","A58"]
[90022029,"A-29,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A29 V-belt Hi-Power II V80 Series. Belt outside circumference length of 31 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 31. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-29","A29","A23"]
[90032031,"B-31,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B31 Hi-Power II V-Belt - 9003-2031. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 34. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-31","B31","A25"]
[90032032,"B-32,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B32 Hi-Power II V-Belt - 9003-2032. Belt Height: 13/32 Belt Top Width: 21/32 \nOutside Circumference (in): 35 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-32","B32","A28"]
[90032041,"B-41,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B41 V-belt Hi-Power II V-Belt - 9003-2041. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 44. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-41",{"$f":"SUBSTITUTE(E68,\"-\",\"\")","v":"B41"},"A57"]
[90032047,"B-47,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B47 V-belt Hi-Power II V-Belt - 9003-2047. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 50. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-47","B47","A59"]
[90032061,"B-61,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B61 V-belt Hi-Power II V-Belt - 9003-2061. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 64. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-61","B61","A60"]
[90032070,"B-70,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B70 V-belt Hi-Power II V-Belt - 9003-2070. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 73. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-70","B70","A61"]
[90032118,"B-118,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B118 V-belt Hi-Power II V-Belt - 9003-2118. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 121. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-118","B118","A63"]
[84002370,"4L-370,GATES(TRUFLEX)BELT","Truflex® V-Belts / Courroies-V TruflexMD Gates Truflex light duty v-belt 4L370 8400-2370.\n4L370 Gates Truflex light duty v-belt 37 inches long x 1/2 top width.Belt Height:  5/16 Belt Top Width:  1/2 Outside Circumference (in): 37 MPN:  4L370",null,"4L-370","4L370","A65"]
[90032058,"B-58,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B58 V-belt Hi-Power II V-Belt - 9003-2058. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 61. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-58","B58","A66"]
[90032062,"B-62,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B62 V-belt Hi-Power II V-Belt - 9003-2062. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 65. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-62","B62","A67"]
[90032063,"B-63,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B63 V-belt Hi-Power II V-Belt - 9003-2063. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 66. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-63","B63","A68"]
[90032073,"B-73,GATES(HI-POWER)BELT GATES V-BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B73 V-belt Hi-Power II V-Belt - 9003-2073. Belt Height: 13/32 Belt Top Width: 21/32\nOutside Circumference (in): 76. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-73","B73","A69"]
[84002380,"4L-380,GATES(TRUFLEX)BELT","4L380 Gates Truflex light duty v-belt 38 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 38. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and \nheat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"4L-380","4L380","A70"]
[90022041,"A-41,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A41 V-belt Hi-Power II V80 Series. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 43. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-41","A41","A72"]
[90022058,"A-58,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A41 V-belt Hi-Power II V80 Series. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 60. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-58","A58","A75"]
[90032043,"B-43,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A43 V-belt Hi-Power II V80 Series. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 46. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-43","B43","A80"]
[90032060,"B-60,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B60 Hi-Power II V-Belt - 9003-2060. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 63. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-60","B60","A85"]
[84002230,"4L-230,GATES(TRUFLEX)BELT","4L230 Gates Truflex light duty v-belt 23 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 23. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-230","4L230","A105"]
[84002260,"4L-260,GATES(TRUFLEX)BELT","4L260 Gates Truflex light duty v-belt 26 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 26. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-260","4L260","A64"]
[84002320,"4L-320,GATES(TRUFLEX)BELT","4L320 Gates Truflex light duty v-belt 32 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 32. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-320","4L320","A112"]
[84002330,"4L-330,GATES(TRUFLEX)BELT","4L330 Gates Truflex light duty v-belt 33 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 33. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-330","4L330","A21"]
[90032083,"B-83,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B83 Hi-Power II V-Belt - 9003-2083. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 86. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-83","B83","A22"]
[90032028,"B-28,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B28 Hi-Power II V-Belt - 9003-2028. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):31. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-28","B28"]
[84001160,"3L-170,GATES(TRUFLEX)BELT","3L160 Gates Truflex light duty v-belt 16 inches long x 3/8 top width. Belt Height: 7/32 Belt Top Width: 3/8 Outside Circumference (in):16. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"3L-170","3L170"]
[84001180,"3L-180,GATES(TRUFLEX)BELT","3L180 Gates Truflex light duty v-belt 18 inches long x 3/8 top width. Belt Height: 7/32 Belt Top Width: 3/8 Outside Circumference (in):18. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"3L-180","3L180"]
[84001200,"3L-200,GATES(TRUFLEX)BELT","3L200 Gates Truflex light duty v-belt 20 inches long x 3/8 top width. Belt Height: 7/32 Belt Top Width: 3/8 Outside Circumference (in):20. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"3L-200","3L200"]
[84002170,"4L-170,GATES(TRUFLEX)BELT","4L170 Gates Truflex light duty v-belt 17 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):17. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-170","4L170"]
[84002180,"4L-180,GATES(TRUFLEX)BELT","4L180 Gates Truflex light duty v-belt 18 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):18. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-180","4L180"]
[84002270,"4L-270,GATES(TRUFLEX)BELT","4L270 Gates Truflex light duty v-belt 27 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):27. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-270","4L270"]
[84002300,"4L-300,GATES(TRUFLEX)BELT","4L300 Gates Truflex light duty v-belt 30 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):30. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-300","4L300"]
[84002310,"4L-310,GATES(TRUFLEX)BELT","4L310 Gates Truflex light duty v-belt 31 inches long x 1/2 top width. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):31. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets RMA oil and heat resistant standards and static conductivity requirements.\n",null,"4L-310","4L310"]
[90022023,"A-23, GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A23 V-belt Hi-Power II V80 Series. Belt outside circumference length of 25 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):25. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-23","A23"]
[90022025,"A-25,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A25 V-belt Hi-Power II V80 Series. Belt outside circumference length of 27 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):27. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-25","A25"]
[90022028,"A-28,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A28 V-belt Hi-Power II V80 Series. Belt outside circumference length of 30 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):30. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-28","A28"]
[90022057,"A-57,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A57 V-belt Hi-Power II V80 Series. Belt outside circumference length of 59 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):59. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-57","A57"]
[90022059,"A-59,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A59 V-belt Hi-Power II V80 Series. Belt outside circumference length of 61 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):61. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-59","A59"]
[90022060,"A60, GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A60 V-belt Hi-Power II V80 Series. Belt outside circumference length of 62 inches.  Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):62. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A60","A60"]
[90022061,"A-61,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A61 V-belt Hi-Power II V80 Series. Belt outside circumference length of 63 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):63. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-61","A61"]
[90022063,"A-63,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A63 V-belt Hi-Power II V80 Series. Belt outside circumference length of 65 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):65. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-63","A63"]
[90022065,"A-65,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A65 V-belt Hi-Power II V80 Series. Belt outside circumference length of 67 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):67. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-65","A65"]
[90022066,"A-66,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A66 V-belt Hi-Power II V80 Series. Belt outside circumference length of 68 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):68. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-66","A66"]
[90022067,"A-67,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A67 V-belt Hi-Power II V80 Series. Belt outside circumference length of 69 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):69. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-67","A67"]
[90022068,"A-68,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A68 V-belt Hi-Power II V80 Series. Belt outside circumference length of 70 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):70. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-68","A68"]
[90022069,"A-69,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A69 V-belt Hi-Power II V80 Series. Belt outside circumference length of 71 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):71. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-69","A69"]
[90022070,"A-70,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A70 V-belt Hi-Power II V80 Series. Belt outside circumference length of 72 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):72. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-70","A70"]
[90022072,"A-72,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A72 V-belt Hi-Power II V80 Series. Belt outside circumference length of 74 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):74. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-72","A72"]
[90022075,"A-75,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A75 V-belt Hi-Power II V80 Series. Belt outside circumference length of 77 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):77. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-75","A75"]
[90022080,"A-80,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A80 V-belt Hi-Power II V80 Series. Belt outside circumference length of 82 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):82. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-80","A80"]
[90022085,"A-85,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A85 V-belt Hi-Power II V80 Series. Belt outside circumference length of 87 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):87. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-85","A85"]
[90022105,"A-105,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A105 V-belt Hi-Power II V80 Series. Belt outside circumference length of 107 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):107. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-105","A105"]
[90022064,"A-64,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates A64 V-belt Hi-Power II V80 Series. Belt outside circumference length of 66 inches. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in):66. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"A-64","A64"]
[90032030,"B-30,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B30 Hi-Power II V-Belt - 9003-2030.  Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):33. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-30","B30"]
[90032033,"B-33,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B33 Hi-Power II V-Belt - 9003-2033. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):36. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-33","B33"]
[90032036,"B-36,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B36 Hi-Power II V-Belt - 9003-2036. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):39. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-36","B36"]
[90032037,"B-37,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B37 Hi-Power II V-Belt - 9003-2037. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):40. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-37","B37"]
[90032039,"B-39,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B39 Hi-Power II V-Belt - 9003-2039. Belt Height: 13/32 Belt Top Width: 21/32Outside Circumference (in):42. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-39","B39"]
[90032045,"B-45,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B45 Hi-Power II V-Belt - 9003-2045. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):48. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-45","B45"]
[90032049,"B-49,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B49 Hi-Power II V-Belt - 9003-2049. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):52. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-49","B49"]
[90032051,"B-51,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B51 Hi-Power II V-Belt - 9003-2051. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):54. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-51","B51"]
[90032052,"B-52,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B52 Hi-Power II V-Belt - 9003-2052. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):55. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n\n",null,"B-52","B52"]
[90032053,"B-53,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B53 Hi-Power II V-Belt - 9003-2053. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):56. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-53","B53"]
[90032054,"B-54,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B54 Hi-Power II V-Belt - 9003-2054. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):57. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n\n",null,"B-54","B54"]
[90032055,"B-55,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B55 Hi-Power II V-Belt - 9003-2055. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):58. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n\n",null,"B-55","B55"]
[90032056,"B-56,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B56 Hi-Power II V-Belt - 9003-2056. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):59. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-56","B56"]
[90032059,"B-59,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B59 Hi-Power II V-Belt - 9003-2059. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):62. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n\n",null,"B-59","B59"]
[90032065,"B-65,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B65 Hi-Power II V-Belt - 9003-2065. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):68. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-65","B65"]
[90032066,"B-66,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B66 Hi-Power II V-Belt - 9003-2066. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):69. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-66",{"$f":"SUBSTITUTE(E132,\"-\",\"\")","v":"B66"}]
[90032068,"B-68,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B68 Hi-Power II V-Belt - 9003-2068. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):71. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-68","B68"]
[90032069,"B-69,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B69 Hi-Power II V-Belt - 9003-2069. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):72. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-69","B69"]
[90032071,"B-71,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B71 Hi-Power II V-Belt - 9003-2071. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):74. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-71","B71"]
[90032072,"B-72,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B72 Hi-Power II V-Belt - 9003-2072. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):75. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-72","B72"]
[90032074,"B-74,GATES(HI-POWER)BELT","Hi-Power® II Belts / Courroies Hi-PowerMD II\nGates B74 Hi-Power II V-Belt - 9003-2074. Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in):77. These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.\n",null,"B-74","B74"]
[90032075,"B-75,GATES(HI-POWER)BELT","Gates B75 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 78 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-75","B75"]
[90032076,"B-76,GATES(HI-POWER)BELT","Gates B76 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 79 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-76","B76"]
[90032077,"B-77,GATES(HI-POWER)BELT","Gates B77 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 80 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-77","B77"]
[90032078,"B-78,GATES(HI-POWER)BELT","Gates B78 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 81 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-78","B78"]
[90032079,"B-79,GATES(HI-POWER)BELT","Gates B79 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 82 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-79","B79"]
[90032080,"B-80,GATES(HI-POWER)BELT","Gates B80 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 83 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-80","B80"]
[90032081,"B-81,GATES(HI-POWER)BELT","Gates B81 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 84 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-81","B81"]
[90032084,"B-84,GATES(HI-POWER)BELT","Gates B84 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 87 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-84","B84"]
[90032085,"B-85,GATES(HI-POWER)BELT","Gates B85 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 88 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-85","B85"]
[90032086,"B-86,GATES(HI-POWER)BELT","Gates B86 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 89 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-86","B86"]
[90032087,"B-87,GATES(HI-POWER)BELT","Gates B87 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 90 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-87","B87"]
[90032089,"B-89,GATES(HI-POWER)BELT","Gates B89 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 92 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-89","B89"]
[90032090,"B-90,GATES(HI-POWER)BELT","Gates B90 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 93 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-90","B90"]
[90032093,"B-93 GATES(HI-POWER)BELT","Gates B93 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 96 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-93","B93"]
[90032094,"B-94,GATES(HI-POWER)BELT","Gates B94 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 97 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-94","B94"]
[90032097,"B97, GATES(HI-POWER)BELT 97\" V-BELT","Gates B97 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 100 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B97","B97"]
[90032105,"B105,GATES(HI-POWER)BELT","Gates B105 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 108 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B105","B105"]
[90032106,"B-106,GATES(HI-POWER)BELT","Gates B106 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 109 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-106","B106"]
[90032108,"B-108,GATES(HI-POWER)BELT","Gates B108 Hi-Power II V-Belt - 9003-2108 Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 111 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-108","B108"]
[90032120,"B-120,GATES(HI-POWER)BELT","Gates B120 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 123 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-120","B120"]
[90032131,"B-131,GATES(HI-POWER)BELT","Gates B131 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 134 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-131","B131"]
[90032136,"B-136,GATES(HI-POWER)BELT","Gates B136 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 139 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-136","B136"]
[90032158,"B-158,GATES(HI-POWER)BELT","Gates B158 Hi-Power II V-Belt Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 161 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-158","B158"]
[90022112,"A-112,GATES(HI-POWER)BELT","Gates A112 V-belt Hi-Power II V80 Series.. Belt Height: 5/16 Belt Top Width: 1/2 Outside Circumference (in): 114 These belts resist oil, heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"A-112","A112"]
[90032082,"B-82,GATES(HI-POWER)BELT","Gates B82 Hi-Power II V-Belt  Belt Height: 13/32 Belt Top Width: 21/32 Outside Circumference (in): 85 These belts resist oil and heat, ozone, sunlight, weather, and aging. Meets ARPM / RMA IP-3-2 oil and heat-resistant standards and ARPM / RMA IP-3-3 static conductivity requirements.",null,"B-82","B82"]
[84002350,"4L-350,GATES(TRUFLEX)BELT","4L350 Gates Truflex light duty v-belt 35 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 35 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-350","4L350"]
[84002390,"4L-390,GATES(TRUFLEX)BELT","4L390 Gates Truflex light duty v-belt 39 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 39 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-390","4L390"]
[84002400,"4L-400,GATES(TRUFLEX)BELT","4L400 Gates Truflex light duty v-belt 40 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 40 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-400","4L400"]
[84002410,"4L-410,GATES(TRUFLEX)BELT","4L410 Gates Truflex light duty v-belt 41 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 41 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-410","4L410"]
[84002420,"4L-420,GATES(TRUFLEX)BELT","4L420 Gates Truflex light duty v-belt 42 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 42 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-420","4L420"]
[84002440,"4L-440,GATES(TRUFLEX)BELT","4L440 Gates Truflex light duty v-belt 44 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 44 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-440","4L440"]
[84002450,"4L-450,GATES(TRUFLEX)BELT","4L450 Gates Truflex light duty v-belt 45 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 45 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-450","4L450"]
[84002460,"4L-460,GATES(TRUFLEX)BELT","4L460 Gates Truflex light duty v-belt 46 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 46 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-460","4L460"]
[84002470,"4L-470,GATES(TRUFLEX)BELT","4L470 Gates Truflex light duty v-belt 47 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in):  47 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-470","4L470"]
[84002480,"4L-480,GATES(TRUFLEX)BELT","4L480 Gates Truflex light duty v-belt 48 inches long x 1/2 top width. Outside Circumference (in): 48 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-480","4L480"]
[84002490,"4L-490,GATES(TRUFLEX)BELT","4L490 Gates Truflex light duty v-belt 49 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 49 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-490","4L490"]
[84002500,"4L-500,GATES(TRUFLEX)BELT","4L500 Gates Truflex light duty v-belt 50 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 50 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-500","4L500"]
[84002510,"4L-510,GATES(TRUFLEX)BELT","4L510 Gates Truflex light duty v-belt 51 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 51 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-510","4L510"]
[84002520,"4L-520,GATES(TRUFLEX)BELT","4L520 Gates Truflex light duty v-belt 52 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 52 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-520","4L520"]
[84002530,"4L-530,GATES(TRUFLEX)BELT","4L530 Gates Truflex light duty v-belt 53 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 53 Suitable for all industrial light duty applications, usually using (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-530","4L530"]
[84002540,"4L-540,GATES(TRUFLEX)BELT","4L540 Gates Truflex light duty v-belt 54 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 54 Suitable for all industrial light duty applications, usually using fractional horsepower (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-540","4L540"]
[84002550,"4L-550,GATES(TRUFLEX)BELT","4L550 Gates Truflex light duty v-belt 55 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 55 Suitable for all industrial light duty applications, usually using fractional horsepower (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-550","4L550"]
[84002560,"4L-560,GATES(TRUFLEX)BELT","4L560 Gates Truflex light duty v-belt 56 inches long x 1/2 top width. Belt Height: 5/16 Outside Circumference (in): 56 Suitable for all industrial light duty applications, usually using fractional horsepower (FHP) motors. Meets RMA oil and heat resistant standards and RMA static conductivity requirements.",null,"4L-560","4L560"]
[94120750,"3VX-750,COGGED V-BELT","Gates 3VX750 Super HC Molded Notch V80 Series V-Belt 3VX Belt Height: 21/64 Belt Top Width: 3/8 Outside Circumference (in): 75 Suitable for all industrial applications, mainly where space, weight and horsepower capacity are critical.",null,"3VX-750","3VX750"]
[94141600,"GATES 5VX-1600 V-BELT","Gates 5VX1600 Super HC Molded Notch V80 Series V-Belt 5VX Belt Top Width: 5/8 Outside Circumference (in): 160 This Belt Has a Superior Combination of Flex and Load Carrying Capacity. Suitable for all industrial applications, mainly where space, weight and horsepower capacity are critical.",null,"GATES","GATES"]
[90022021,"A-21 GATES HI-POWER BELT","Featuring a composite, multi-purpose construction, these belts resist oil and heat, ozone, sunlight, weather, and aging. Gates A21 V-belt Hi-Power II V80 Series. Belt outside circumference length of 23 inches. Belt Height: 5/16 Belt Top Width: 1/2",null,"A-21","A21"]
[90032124,"B-124,GATES(HI-POWER)BELT","Featuring a composite, multi-purpose construction, these belts resist oil and heat, ozone, sunlight, weather, and aging. Gates B124 Hi-Power II V-Belt Belt Height:  13/32 Belt Top Width:  21/32 Outside Circumference (in):  127",null,"B-124","B124"]
[90022022,"A-22 GATES HI-POWER BELT","Featuring a composite, multi-purpose construction, these belts resist oil and heat, ozone, sunlight, weather, and aging. Gates A22 V-belt Hi-Power II V80 Series. Belt outside circumference length of 24 inches. Belt Height:  5/16 Belt Top Width: 1/2",null,"A-22","A22"]

{"sheet":"Sheet5","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}